[codec]
.m4b
fdkaac.exe

[label]
4
2
Target:


[radio&slider]
4
24
292
2
40
0
Quality (VBR)

5
Quality 1   (estimated bit rate: 64 Kbps)
-m 1
Quality 2   (estimated bit rate: 80 Kbps)
-m 2
Quality 3   (estimated bit rate: 96 Kbps)
-m 3
Quality 4   (estimated bit rate: 144 Kbps)
-m 4
Quality 5   (estimated bit rate: 224 Kbps)
-m 5
[/sliderend]
110
0
Bit Rate (CBR)

15
Bit Rate: 8 kbps
-b 8
Bit Rate: 12 kbps
-b 12000
Bit Rate: 16 kbps
-b 16000
Bit Rate: 24 kbps
-b 24000
Bit Rate: 32 kbps
-b 32000
Bit Rate: 48 kbps
-b 48000
Bit Rate: 56 kbps
-b 56000
Bit Rate: 64 kbps
-b 64000
Bit Rate: 80 kbps
-b 80000
Bit Rate: 96 kbps
-b 96000
Bit Rate: 128 kbps
-b 128000
Bit Rate: 144 kbps
-b 144000
Bit Rate: 160 kbps
-b 160000
Bit Rate: 192 kbps
-b 192000
Bit Rate: 224 kbps
-b 224000 -w 22050
Bit Rate: 256 kbps
-b 256000 -w 22050
Bit Rate: 320 kbps
-b 320000 -w 22050
Bit Rate: 400 kbps
-b 400000 -w 22050
Bit Rate: 480 kbps
-b 480000 -w 22050
Bit Rate: 512 kbps
-b 512000 -w 22050
[/sliderend]







[label]
10
44
low quality (smaller file)
808080

[label]
216
44
high quality (larger file)
808080

[combo]
60
66
120
1
LC AAC
 -p 2
HE AAC (below 96 kbps)
 -p 5  
HE v2 AAC (below 56 kbps)
 -p 29  



[clistring]
 --ignorelength -S -o "[outfile]" - 

[highestqualitydecode]


[minfreq]
8000

[maxfreq]
96000

[maxchannels]
6


[helpbutton]
283
0
Help\dMC\m4a (AAC).html

[estimatesize]
-b 512000
512000
-b 480000
480000
-b 400000
400000
-b 320000
320000
-b 256000
256000
-b 224000
224000
-b 192000
192000
-b 160000
160000
-b 144000
144000
-b 128000
128000
-b 96000
96000
-b 80000
80000
-b 64000
64000
-b 56000
56000
-b 48000
48000
-b 32000
32000
-b 24000
24000
-b 16000
16000
-b 12000
12000
-b 8000
8000
-m 1
64000
-m 2
80000
-m 3
96000
-m 4
144000
-m 5
224000
